**True/false**

1. LTU can be connected between ETC to ETC. (True/**False**)
2. LIU can be connected to ETC to ETC line commn. (**True**/False)
3. ATD keys are generated by KGU software. (**True**/False)
4. ETD keys are generated by KTU software. (**True**/False)
5. RIA binding post is used for line communication of ETC. (True/**False**)
6. Li Ion rechargeable Bty of HHC MK-II have 7.3 volt 2.4 AH (True/**False**)
7. LIU can be connected to any Radio port of ETC MK-II (True/**False**).
8. LTU required 12 Volts DC power input (True/**False**).
9. ETC required 12 Volts DC power input (True/**False**).
10. Flash memory of HHC 1GB (True/**False**)