|  |  |
| --- | --- |
| S No | **SCANNER** |
| 1 | CCD stand for ? |
| ANS | Charged couple device. |
| 2 |  |
| ANS |  |
| **FAX** | |
| 1 | Out put voltage of power supply unit ? |
| Ans | 22V,18 and 4.5 V (Printer,scanner,ics) |
| 2 | Thermal printing page made up by which material ? |
| Ans | Fluoranleucodye and Octadecyl fosphonic acid |
|  |  |
|  | **DOT MATRIX PRINTER** |
| 1 | Power supply out put voltage? |
| Ans | 5 v Electonic cct, -12 buffer , 24 v for Head and stepper motor |
| 2 | Head home posn sensor use for ? |
| Ans | Correct posn of head where print start |
|  | **INKJET PRINTER** |
| 1 | Main function of encoder strip ? |
| Ans | Control the movment of printing head |
| 2 | Function of Encoder disc ? |
| Ans | Control the movement of paper |
|  |  |
|  |  |
|  | **LASER JET PRINTER** |
| 1 | OPC Drum made by which material ? |
| Ans | Aluminum cylinder with semiconductor coating (selenium and zink oxide) |
| 2 | All sensor operated voltage ? |
| ans | 3.3 V |
| 3 | Solonoid sw operating voltage ? |
| Ans | 24 V |
| 4 | Printer Show in off line mode ? |
| Ans | Dada cable, printer port section |
|  |  |
|  |  |
|  |  |